**MWM TCG 2016 V8**

Original MWM® knock sensors, 2 per engine bank.

The following sensor inputs at DetCon20 need to be bridged

English:

|  |  |  |
| --- | --- | --- |
| **Firing order** | **Sensor input DetCon** | **Bridge inputs** |
| A1 | 1 | 1+7\* |
| B2 | 2 | 2+4\* |
| A3 | 3 | 3+5\* |
| B1 | 4 | 4+2 |
| A4 | 5 | 5+3 |
| B3 | 6 | 6+8\* |
| A2 | 7 | 7+1 |
| B4 | 8 | 8+6 |